--Notes on how to get run the thrustmaster force feedback wheel.

  In order to run with the force feedback wheel you will need to run xcar with the
-F command line switch.  Currently the game will not be able to re-start the HAPTIC
library so the game will have to be completely exited and re-started each time the library
is initialized and closed.  This happens in joystick calibration, control selection and
during a race.  I am assuming you know how to set up the com port in the citwheel.nmr
file.

  Most of the effects we have set up use frequency, magnitude and duration values which
may be adjusted by editing the wheel.des text file.  These values are integers which will
be divided by 10 to form fractions.  Maximum force for the wheel is .6 so higher numbers
may not make a noticable difference in wheel performance.

  If you have any technical problems call me at 360-493-1348 during Pacific time 9:00 am
to 6:00 pm. or send E-Mail to GCarver@mtwest.com.